Filter Definition File
For each Channel, N is the width (in seconds) of the sliding window in each direction from the central sample
Channel                  N
&START  V1.t
GRST-GR                  0
GRST-Temp                0
GRST-5V                  0
GIST-RawRateX            0
GIST-RawRateY            0
GIST-RawAcelX            0
GIST-RawAcelY            0
GIST-TempG               0
GIST-TempAX              0
GIST-TempAY              0
GIST-TempADCX            0
GIST-TempADCY            0
GIST-RateX               0
GIST-RateY               0
GIST-AcelX               0
GIST-AcelY               0
GIST-DEVI                0
GIST-HAZI                0
GIST-TFACE               0
GIST-RB                  0
SPINNER-RPS              0
SPINNER-INVERTEDRPS      0
SPINNER-5V               0
SPINNER-Temp             0
PSST-PT100               1
PSST-PTemp               0
PSST-Pressure            0
PSST-5V                  0
PSST-CCL1                0
PSST-CCL2                0
PSST-CCL3                0
PSST-CCL4                0
WHST                     0
WHST-5V                  0
WHST-Temp                0
BMST-HVolt               0
BMST-HCurr               1
BMST-Temp                0
BMST-BVolt               0
&END