WSS Tool List Definition. Please read the instruction manual in order to know how to
apply changes to this structure (only for upgrading purposes)

&STARTLIST
TCST-B
BMST
GRST-B
GIST-A
GIST-B
GIST-B(FLASKED)
GIST-C
GIST-C(FLASKED)
SCST-B
PSST-B
WHST-A
WDLT
ECCL
GUNC
&ENDLIST
&STARTACSESORY
**HEAD
**HADAPTER
**CENTRALIZER
**B-NOSE
**ILC-A
**SAA
&ENDACSESORY

Tool porccess data structture definition
There must be a structure definition per each tool listed above

&STARTSTRUCT
&TCST-B
TCST-B
3
3
254
1
54.5
42.8
0
0
1
&BMST
BMST
3
3
251
1
70
42.8
0
0
1
&GRST-B
GRST-B
3
2
210
1
76.6
42.8
0
0
1
&GIST-A
GIST-A
17
5
220
3
107
42.8
0
0
1
&GIST-B
GIST-B
24
19
224
3
138.5
42.8
0
0
1
&GIST-B(FLASKED)
GISTB-FSK
24
19
224
3
209
42.8
0
0
1
&GIST-C
GIST-C
24
19
224
3
138.5
42.8
0
0
1
&GIST-C(FLASKED)
GISTC-FSK
24
19
224
3
209
42.8
0
0
1
&SCST-B
SCST-B
6
4
230
1
34.5
42.8
0
0
1
&PSST-B
PSST-B
16
9
232
2
65.0
42.8
0
0
1
&WHST-A
WHST-A
6
4
235
1
56.0
42.8
0
0
1
&WDLT
WDLT
3
4
240
3
53
42.8
0
0
1
&ECCL
ECCL
2
1
252
1
45
45.72
0
0
1
&GUNC
GUNC
0
0
0
0
200
60
0
0
1
&**HEAD
HEAD
0
0
0
0
45
42.8
0
0
2
&**HADAPTER
ADAPTER
0
0
0
0
14.5
42.8
0
0
3
&**CENTRALIZER
CENTRALIZER
0
0
0
0
40
42.8
0
0
4
&**B-NOSE
B-NOSE
0
0
0
0
5
42.8
0
0
5
&**ILC-A
ILC-A
0
0
0
0
63.5
42.8
0
0
6
&**SAA
SAA
0
0
0
0
31.5
42.8
0
0
7
&ENDSTRUCT

Channel offsets for each tool sensor
Values in mm from the bottom of the tool

&STARTCHANNEL
PSST-PT100
130
PSST-PTemp
154
PSST-Pressure
154
PSST-CCL1
520
PSST-CCL2
520
PSST-CCL3
520
PSST-CCL4
520
WHST
145
GRST-GR
165
&ENDCHANNEL
&END
